|  |  |  |
| --- | --- | --- |
| **Invisible Fence® Brand Product Info & Compatibilities** | | |
| ICT725 Outdoor Transmitter  IF ICT725 Transmitter.jpg   * Platinum Series Product * Battery Backup Compatible * Covers up to 12 acres (3000')   Compatibility: **A** | R21 Platinum Series Receiver  C:\Graphics & Photos (Work)\Pet Containment Equipment\Receivers\Invisible Fence R21P NEW (words).jpg   * Weighs 1.6 oz. * Water resistant * 7K or 10K Programmable * Four Static Correction Levels * Requires PowerCap style battery★   Compatibility: **A** | R5000 Receiver  C:\Graphics & Photos (Work)\Pet Containment Equipment\Receivers\Invisible Fence R5000.jpg   * Original Receiver - Weighs 3.8 oz. * 7K or 10K, Not Programmable * One correction level * Requires 7.5v Silver Oxide Battery   Compatibility: **A** |
| ICT700 Outdoor Transmitter  C:\Graphics & Photos (Work)\Pet Containment Equipment\Transmitters\IF ICT700 Transmitter.jpg   * Platinum Series Product * 7K or 10K Switchable * Covers up to 12 acres (3000')   Compatibility: **A** | Perimeter® ComputerReceiver™  C:\Graphics & Photos (Work)\Pet Containment Equipment\Receivers\PT R22 IF Rx Collar.gif   * Weighs 1.1 oz. * Low Battery Warning Light * 7K or 10K Programmable * 4 Static + 1 Prog Corrections * Requires 6v Lithium Battery   Compatibility: **A** | R6500 Receiver  C:\Graphics & Photos (Work)\Pet Containment Equipment\Receivers\Invisible Fence R6500 Rx.jpg   * Weighs 2.7 oz. * 7K or 10K, Not Programmable * One correction level * Requires 7.5v Silver Oxide Battery   Compatibility: **A** |
| ICT801 Outdoor Transmitter  C:\Graphics & Photos (Work)\Pet Containment Equipment\Transmitters\IFPS ICT801 Tx 2.jpg   * Titanium Series, * 7K or 10K, I/O Switchable * Battery Backup Compatible * Available w/Dual Loop Capability   Compatibility: **B** | R21 Titanium Series Receiver  C:\Graphics & Photos (Work)\Pet Containment Equipment\Receivers\Invisible Fence R21Tv4.jpg   * Weighs 1.6 oz. * Water resistant * 7K/10K, I/O Programmable * Newer version, more options * Requires PowerCap style battery★   Compatibility: **B** | MicroLite™ Receiver  C:\Graphics & Photos (Work)\Pet Containment Equipment\Receivers\Invisible Fence MicroLite.jpg   * Weighs 1.0 oz., Waterproof * 7K/10K, I/O Programmable * Functions same as Titanium R21 * Requires PowerCap style battery★ * Colorful removable 'skins'   Compatibility: **A** or **B** |
| ICT150 Outdoor Transmitter  C:\Graphics & Photos (Work)\Pet Containment Equipment\Transmitters\IF ICT150 Transmitter.jpg   * Similar Predecessor of ICT700 * 7K or 10K Switchable * Covers up to 12 acres (3000') * ICT100/100A are Non-switchable   Compatibility: **A** | R21 Mink Series Receiver  C:\Graphics & Photos (Work)\Pet Containment Equipment\Receivers\Invisible Fence R21P NEW (logo).jpg   * Weighs 1.6 oz. * Water resistant * 7K or 10K Programmable * Older version, fewer options * Requires PowerCap style battery★   Compatibility: **A** | LP3000 Loop Lightning Protector  C:\Graphics & Photos (Work)\Accessories & Wire\IF LP3000.jpg   * Identical to older Blue Version * Protects Boundary Loop only   Compatibility: **U** |
| Invisible Gate Outdoor Transmitter  C:\Graphics & Photos (Work)\Pet Containment Equipment\Transmitters\IF Gate Tx.jpg   * Similar to ICT75 * 7K or 10K Switchable * Covers up to ~1/2 acre (500')   Compatibility: **A** | R21 Graphite Series Receiver  C:\Graphics & Photos (Work)\Pet Containment Equipment\Receivers\Invisible Fence R21G NEW (words).jpg   * Weighs 1.6 oz. * Water resistant * 7K or 10K Programmable * Same as Platinum, Less Warranty * Requires PowerCap style battery★   Compatibility: **A** | LP4100 Lightning & Surge Protector  C:\Graphics & Photos (Work)\Accessories & Wire\IFLP4100.jpg   * Identical to Innotek Version * Protects Boundary Loop & Power Supply   Compatibility: **U** |
| ICT750 (250) Outdoor Transmitter  IF ICT725 Transmitter.jpg   * Platinum Series, 7K or 10K Switch * Battery Backup Compatible * Dual Independent Loop Capable   Compatibility: **A** | R51 Platinum Series Receiver  C:\Graphics & Photos (Work)\Pet Containment Equipment\Receivers\Invisible Fence R51P (New Logo).jpg   * Weighs 1.6 oz. * Water resistant * 7K or 10K Programmable * For use with stubborn pets * Requires PowerCap style battery★   Compatibility: **A** | Battery Backup Unit  C:\Graphics & Photos (Work)\Accessories & Wire\IF Battery Box.jpg   * Houses 12v Rechargeable Battery * Includes Wiring Harness   Compatibility: **I** |
| ICT775 Outdoor Transmitter  IF ICT725 Transmitter.jpg   * Platinum Series, 7K Only * Battery Backup Compatible * For Large Yards (up to 35 acres) * 3-Sided Loop Capable   Compatibility: **A** | IFA12 Indoor Avoidance Unit  C:\Graphics & Photos (Work)\Pet Containment Equipment\Transmitters\IFA12 Indoor Tx.jpg   * 7K or 10K Switchable * Must be plugged in to A/C power * Range Adjustable to ~6' Radius   Compatibility: **A** | Shields™ Indoor Avoidance Unit  C:\Graphics & Photos (Work)\Pet Containment Equipment\Transmitters\IFSHIELDS.jpg   * 7K or 10K, Indoor/Outdoor Switchable * Battery Operated (rechargeable) * Range Adjustable to ~6' Radius   Compatibility: **B** |
|  | | |
| **COMPATIBILITY DESIGNATIONS AND NOTES:**   * **A** – Compatibility Group includes all Invisible Fence brand 100 or 700 series outdoor transmitters, as well as all R21/R51/A12 Receivers except the Titanium versions. Fully compatible with the Perimeter ComputerReceiver. Not compatible with 800 series outdoor transmitters or Shields Indoor units. **Further Note:** This group is also compatible with Pet Stop® brand pet fence equipment, using Pet Stop’s firmware programming settings. Only the IFA12 in this group is incompatible with Pet Stop receivers. * **B** – Compatibility Group includes 800 series outdoor transmitters, R21 Titanium receivers, MicroLite™ receiver, and Shields™ Indoor units. Not compatible with 100 or 700 series outdoor transmitters or IFA12 Indoor unit, or Perimeter ComputerReceiver, or Pet Stop brand transmitters and receivers. * **I** – Compatibility Group includes all Invisible Fence brand outdoor transmitters with internal battery backup circuitry. These include the ICT725, ICT250/750, ICT775, and ICT801/802. * **U** – Compatibility Group includes all wired pet containment transmitters, including all brands.   ★– Will accept either the Perimeter brand R21 Replacement battery (formerly Pet Stop brand) or the Invisible Fence brand Powercap battery. *(The uncommon Invisible Fence brand R22 receiver, which is larger than the R21, will accept only the Invisible Fence brand Powercap battery and not the Perimeter brand version.)*  Perimeter R21 Battery.jpgALL Invisible Fence brand receivers are also compatible with any Perimeter brand Contact Posts. | | |
| **InvisibleFenceCompatible.com** | | |